**OPERATION PROCEDURE OF INITIALIZING GSM MODEM AND FEEDING THE PHONE NUMBER**

1. **Select a SIM which has got Good Network coverage.**
2. **Place the SIM into GSM modem, Ensure the SIM has got enough money to send SMS.**
3. **Kindly Ensure You Don’t Need Any OF The SMS Stored In The SIM Card As They Will Be Deleted**
4. **Check power led (red color) glowing, See for Network LED (mostly Green color) blinking faster.**
5. **Wait for 2 minutes and one can observe Network LED blinking a bit slower...Indicates SIM has got network coverage.**
6. **Now Press the RESET button at the device, and one can see the “Testing GSM Modem” on LCD.**
7. **If not then Check Modem connection And RESET The Microcontroller**
8. **Then the Display should show “Kindly Call”, it is the process to save the number to which SMS should receive.**
9. **Then give a call from the number (to which SMS should receive) to the Number present in the GSM modem and observe the LCD, The call will disconnect automatically.**
10. **You can observe the mobile number on the LCD.**
11. **If it not able to display the number then RESET the device and follow the Steps from 6 until the number displays.**
12. **This ends the process of initializing GSM modem and feeding the phone number.**